{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["施工","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"施工","index":0,"n_rows":7,"n_cols":7,"rows_kept":7,"merged":[[0,0,0,6],[1,0,1,6],[5,0,5,5],[6,0,6,6]]}
["招标控制价"]
["项目名称：南昌市红谷滩区投书浦公园、老丰和电排站前池补水工程-拖拉管劳务作业"]
["劳务作业内容 ","规格型号","单位","暂定数量","税率","综合单价\n（元）","总价\n（元）"]
["聚乙烯PE100管水平导向钻进回拖布管作业，满足按设计图纸施工验收要求：\n1、水平导向钻进、钻导向孔 DN≤300mm\n2、水平导向钻进扩孔(mm以内)DN300\n3、回拖布管HDPE PE100平壁管DN200\n4、管道消毒冲洗液压试验\n5、泥浆罐车运淤泥流砂\n6、围挡、围堰等安全文明施工措施\n7、其他必要辅助性措施","De200\n公称压力≥1MPa，国标","m",72,{"v":0.03,"d":"3%"},210,{"$f":"D4*F4","v":15120}]
["聚乙烯PE100管水平导向钻进回拖布管作业，满足按设计图纸施工验收要求：\n1、水平导向钻进、钻导向孔 DN≤600mm\n2、水平导向钻进扩孔(mm以内)DN500\n3、回拖布管HDPE PE100平壁管DN400\n4、管道消毒冲洗液压试验\n5、泥浆罐车运淤泥流砂\n6、围挡、围堰等安全文明施工措施\n7、其他必要辅助性措施","De400\n公称压力≥1MPa，国标","m",1450,{"v":0.03,"d":"3%"},{"$f":"557","v":557},{"$f":"D5*F5","v":807650}]
["合计（元）：",{"$nulls":5},{"$f":"SUM(G4:G5)","v":822770}]
["注：1、劳务作业单价为含管理费利润、税费、风险费等一切费用；招标数量为按图纸理论计量，据实结算。\n"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}